**Week 2 graded quiz**

**LATEST SUBMISSION GRADE**

100%

1.Question 1

Applications running on an operating system through a simplified series of interfaces is referred to as Application programming interfaces



True



False

**Correct**

**1 / 1 point**

2.Question 2

What is the minimum number of LPARs in a Sysplex?



16



2



1



32

**Correct**

**1 / 1 point**

3.Question 3

Which z/OS component manages communications between applications in a Parallel Sysplex?



Hipersockets



Cross-system coupling facility



VTAM



TCP/IP

**Correct**

**1 / 1 point**

4.Question 4

Which z/OS component is used for managing workload distribution, workload balancing, and distributing resources to competing workloads?



Resource control



Workload manager



Workload distribution



Resource balancing

**Correct**

**1 / 1 point**

5.Question 5

What's the most accurate definition of a Network Interface Card (NIC)?



A NIC moves information directly from the computer to computers on the internet.



A NIC is a computer hardware component that connects a computer to a network.



A NIC comprises of the hardware and software components that connects the RJ-15 cable to the RJ-45



A NIC controls the flow of information from the IP to the TCP, over hardware and software.

**Correct**

**1 / 1 point**

6.Question 6

What does VSAM stand for?



Virtually Stored Accessories Methodology



Virtual Storage Access Method



Virtual Safe Access Method

**Correct**

**1 / 1 point**

7.Question 7

Which is the best definition of a console as it pertains to Mainframe?



A user interface to a server, for example, the interface provided on a personal computer.



A collection of optional software features, with a web-browser interface, that is used for configuring, managing, and monitoring data-copy functions.



A​ screen that resides within the computer.

**Correct**

**1 / 1 point**

8.Question 8

What's the best definition of an LDAP?



Defines a standard method to access and update information in a directory.



A semiconductor chip that displays visible or infrared light when activated.



A set of system commands, library routines, and other tools that allow the user to establish and control logical volume storage.

**Correct**

**1 / 1 point**

9.Question 9

W​hat does GDPS stand for?



Geographically Dispersed Parallel Sysplex



Graphic DiPlo Sysplex



G​eomegric Duplicity Parallel Sysplex